Building an Open Source IoT Garage Controller

|  |  |
| --- | --- |
| Daniel A. Zajac  Department of Electrical and Computer Engineering  University of Michigan  danzajac@umich.edu | Jackson Harmer  Department of Electrical and Computer Engineering  University of Michigan  jharmer@umich.edu |

*Abstract*— Internet connected technologies have become mainstays of the modern household. From Internet of Things (IoT) connected coffee makers to sophisticated adaptive climate control systems, inexpensive wireless technology and popularity of voice activated digital assistants has enabled a wide variety of connected tech. Most of this technology remains closed source however. Many of the more popular connected technologies, such as Nest or ecoBee, rely on closed source protocols and cloud service backends. What happens when these companies go out of business or shut down older services? VueZone shut down its services leaving owners with severely crippled expensive IoT cameras. [1] This paper focuses on building a proof of concept IoT connected garage door real time controller and fully published interface and source: The GarageRTC! This paper reviews the features, design, and implementation of a reference architecture built on an ESP32 microcontroller built on FreeRTOS software as well as performance and possible future improvements.

Keywords—GarageRTC, IoT, Embedded, FreeRTOS, ESP32, NodeMCU, RTOS

# Introduction

As IoT become more common place in our daily lives we become increasingly dependent on the connected services that support those systems. Some of the more popular devices, such as Nest thermostat, are the product of small teams operating as a startup. As these teams grow they are sometimes bought out by larger corporations interested in entering into the IoT market. For some less fortunate start‑ups, they never break through into profitability and slowly descend into obscurity.

What happens to the devices that depend on the cloud services previously maintained and supported by those teams? Sometimes they can continue to function but with crippled or limited performance. Often, they are rendered useless as registration and web-based configuration tools become obsolete. [2] For inexpensive devices, they can be cannibalized for parts or simply disposed of. For more expensive equipment, such as the Juicero, the founding company dissolved leaving many users with useless $400 IoT juice machines. [3]

The only guaranteed way to ensure these devices can be indefinitely supported is to implement an open source methodology including web APIs. Preferably, a completely open source hardware and software reference design would be created and published. Startups wishing to develop derivative works, could leverage the technology could then extend the designs. If the startup dissolves or can no longer support their design, if compatibility with the reference design was maintained, an internet user community would be able to continue support. This concept has been demonstrated profitable and sustainable in large software efforts such as IBM supported Red Hat Linux. [4]

To prove out this concept, the research team designed and built a reference design for an IoT connected Garage real time system, or simply, the GarageRTC.

The GarageRTC is an automation system for a consumer garage connected as an IoT device, Figure 1. The system makes the status of garage available to the user connected remotely through a web-based interface or locally via a display and control panel. Inside the garage, the system is connected to the garage door opener, a garage light, and an alarm. The system uses sensors to detect door position, accumulation of carbon monoxide, temperature, and objects in the path of the door. The user can check the status or manipulate the controls from the control panel or web interface.




Figure 1. GarageRTC Concept

This paper documents the design process, development, implementation, and testing of a WiFi connected garage monitoring system. It implements a basic JSON based API and includes a reference web application that can easily be hosted in a personal cloud or Linux based development board.

## Organization of this Paper

This paper is organized into ten parts:

* **Introduction** – Introduces the motivations and organization of this project.
* **Objectives and Functional Description** – Outlines the high-level objectives for the project and reviews the design process employed.
* **Requirements** – Reviews the high-level requirements the GarageRTC was designed to meet.
* **High Level Design** – Describes the process used to decompose and partition the system and generate high level designs and test plans.
* **Detail Design** – Discussion on the detailed design decisions including selection of hardware, software, and web application.
* **Testing** – Review of the tests and stages used to ensure proper functioning of the system.
* **Accomplishments** – Review of the objectives met, limitations of the current design, possible improvements, and lessons learned.
* **Comparison of Commercial Offerings** – A comparative discussion about similar products commercially available.
* **Conclusions and Closing Remarks**
* **References**

# Objective and Functional Description

The objective of the GarageRTC project was to develop an open source real-time embedded system that can be integrated with an existing opener system. The GarageRTC collects data from obstruction detectors, limit switches, carbon monoxide (CO) concentration, and temperature. It maintains a connection to a basic web server. From the control panel or web interface, the user can observe the following:

* Status of the garage door (open, moving, or closed)
* Status of the light (on or off)
* Level of carbon monoxide
* Temperature in the garage
* Errors or Messages

From either interface, the user can execute commands including:

* Open or Close the door
* Stop door movement
* Turn on/off the Light
* Silence the alarm

The system monitors the environmental conditions of the garage and can sound an alarm if the any of the following issues are detected:

* Carbon Monoxide level too high
* Low temperature/freezing risk
* High temperature/possible fire
* Movement of the door interrupted by an object

This system provides the user an easy way to operate and monitor and control the status of their garage. The scope of this effort it to create the garage interface control and status architecture and basic web interface.

## Design Process

This project was developed using a waterfall software development lifecycle. Adherence to a classic waterfall model was attempted, but during implementation it was discovered that the original display selected was not functioning properly. The display originally selected, a .72 in OLED, had partially implemented drivers and the display was smaller and more difficult to read than expected. The team returned to the design phase briefly to select another display that met the requirements and had better driver support. The waterfall software development lifecycle with the feedback into the design phase is illustrated in Figure 2.




Figure 2. Waterfall Software Development Lifecycle

The maintenance phase is not applicable in this instance as this paper represents the final stage of this effort. The team did make several recommendations for follow on improvements and the source is available in the public GitHub repository. The proposed improvements can be found in section VII of this paper.

# Requirements

The high-level requirements were developed as part of the initial project proposal paper during the concept portion of the design process. Functionally the system needed to have the following interfaces:

* Electrical interface with a garage door opener
* Electrical interface with a mains voltage light
* Web interface for remote operation
* CO and temperature monitoring
* Limit switches and obstacle detection
* Local display and buttons

Design detail within the system was mostly left up to the design activity but was loosely defined as a conventional web server interfaced to the embedded system. Further detail was provided on the specific functions of each button and the display content. The web display would mirror the local display and provide buttons to interact with the embedded system as if the user was local. Response timing goals was also provided and are summarized in Table 1.

Table 1. Response Timing Goals

| **Parameter** | **Timing Requirement** |
| --- | --- |
| Local Display | Every 500 mS or better |
| Obstacle Detection | Toggle opener within 150 mS from detection |
| Limit Switch | Toggle opener within 150 mS from detection |
| Door movement | Toggle opener within 300 mS from press |
| Light | Latch light within 300 mS from press |
| Idle Post to Server | Post to the server every 5000 mS |
| Event push to server | Post to the server within 500 mS from event. |
| Check Server | Check remote messages every 1000 mS |

From the timing goals and requirements, a system block diagram, Figure 3, was composed to illustrate the major partitioning of the system and the system inputs and outputs. The block diagram was annotated to show the type of signal (resistive, digital, voltage, UDP data, etc…) and the response times for outputs.




Figure 3. GarageRTC System Block Diagram

# High Level Design

From the block diagram, the major partitioning of the system could be determined. The functions of the internet server were could be developed independently from the embedded system assuming good interface constraints could be established between the two. Since this project team was not regionally co-located, this made for a good way of separation of efforts. Figure 4 shows the decomposition of functions and responsibilities of entire system. This section reviews the activities performed as part of the high-level design for the GarageRTC project.




Figure 4. GarageRTC System Organization

## Interface specification

To enable independent development of the embedded system and web service, a simple JSON based messaging interface was developed. Three different packets were identified embedded status, status request, and send command. These commands would be sent over ethernet protocol using UDP and encoded in a plaintext JSON formatting. Examples for the EmbeddedStatus, StatusRequest, and SendCommand are show in Figure 5, Figure 6, and Figure 7 respectively.

*{ {"name": "alarmStatus", "value": "False"},*

*{"name": "doorStatus", "value": "2"},*

*{"name": "lightStatus", "value": "OFF"},*

*{"name": "tempStatus", "value": " 63.4"},*

*{"name": "coStatus", "value": "LOW"}*

*}*

Where doorStatus value equals:

0x0 = OPEN 0x1 = CLOSE

0x2 = STOP 0x3 = MOVE

Figure 5. EmbeddedStatus Packet

*{"cmd": "getStatus", "arg": ""}*

Figure 6. StatusRequest Packet

The SendCommand and EmbeddedStatus packets used a bitwise encoding of the command value to the encode enumerations of the door position status and the command type. This simplified the design on the embedded side and required less string work within the limited resources of the microcontroller.

*{ CMD:<value> }*

Where <value> equals:

0x1 – Door Command

0x2 – Light Command

0x4 – Alarm Command

Figure 7. SendCommand Packet

The downside of this formatting is it required the embedded side to do string work to compose and receive the messages from the web server. The embedded system turned out to have ample resources, both memory and speed, to accomplish crafting and processing of these messages. The benefits of this format was the web services side could easily consume the JSON format and there was less chance of interpretation error.

## Embedded System

For the embedded system, a real-time OS was necessary to provide predictable response to inputs while simultaneously executing multiple tasks in a timely fashion. While scratch development of a RTOS was considered, ultimately the FreeRTOS project was selected. FreeRTOS implements a real-time kernel and schedulers targeted as low resource microcontrollers. The project is professionally developed and is available for free use in commercial embedded systems. It supports a wide variety of hardware and offers excellent documentation and, most importantly, is freely available including source. [5]

The Espressif ESP series of embedded microcontrollers was selected as primary controller for the embedded system. This controller has rich library support and, most importantly, an integrated Wi-Fi transceiver. This would enable the embedded system to be built physically separate from the web server. The embedded application would be built in C++/C as this is the language the FreeRTOS and Espressif libraries are developed to support. [6] The Arduino IDE was also selected as it offers integration with the Espressif, FreeRTOS, and a variety of development support tools rolled into a convenient to use environment.

## Web Application

The web application needed to accomplish a fairly simple function, process packets to and from the embedded system and post them to a web page. While this conceptually sounds very simple, it ended up involving several different projects to achieve the desired result. The research team did not want a page that was continually refreshing and made the decision that the page would dynamically update. The content should remain the same without forcing the browser to go through continually updating cycles. In the background, a combination of JavaScript and HTML would fetch and update components of the page dynamically.

The team composed a data flow graph to illustrate the data flow through the web component. The web subsystem would need to present a page in HTML format, process interactions from the user, packets sent via UDP from the embedded system, and convert user clicks into commands to the GarageRTC. The simplest toolchain to achieve this function would be a combination of a web server for hosting, Cascading Style Sheets (CSS), and Javascript for dynamically updating. Python would act as a go-between consuming and converting data and storing the data structures and invoking behaviors.

Since the web application was not the primary focus of this effort, several decisions were made to simplify the design. First, rather than a complete web server stack Flask was selected to implement the python, JavaScript, and HTML frontend. [7] Flask is a microframework with integrated server that is useful for rapid prototyping of python-based transaction framework. It dynamically creates web content based on python models and incorporates an integrated web server.

The second design decision was to use socketio for handling the dynamic behavior of the web page. [8] Socketio enables client-server interactive behavior built on JavaScript. Socketio integrates well with Flask and enabled the resulting page to dynamically update the system status without constant refreshing.

## Documentation

During the Design phase, two documents were initiated, the initial draft of the product manual, and the test plan created. The draft manual helped to outline how the team expected the user to interact with the GarageRTC. The manual was then iteratively updated through the design, implementation, and testing phases. The final manual is available on the project website.

The test plan was a simple matrix that listed the various stages of testing to be performed and mapped them to the requirements established early on. The test plan is summarized below. Testing was broken into three parts: embedded, web, and complete system. The test level (L) indicates U, I, F, or A which are defined as follows:

* U – Unit Level Testing
* I – Integration Testing
* F – Functional Testing
* A – Acceptance Testing

Table 2. Embedded System Test Plan

| **#** | **L** | **Description** | **Tests function:** |
| --- | --- | --- | --- |
| 1E | U | Board functional | Basic I/O, IDE, toolchain |
| 2E | U | Display | LCD Driver, Text, Display Task |
| 3E | U | A/D sensing | AD conversion, scaling |
| 4E | U | CO | CO sensor, Calibration |
| 5E | U | Temperature | Temperature, Calibration |
| 6E | U | Relay | Relay module, I/O driver |
| 7E | U | Limit Switches | Switch input |
| 8E | U | Buttons | Button input |
| 9E | U | Network | Associate, receive, send UDP |
| 10E | U | Alarm Logic | State machine for Alarm control |
| 11E | U | Light Logic | State machine for Light control |
| 12E | U | Door Logic | State machine for Door control |
| 13E | U | FreeRTOS | Scheduler, library compatibility |
| 14E | U | Shared Memory | Globals, mutexes, semaphores |
| 15E | I | Network Commands | Send/Receive commands |
| 16E | I | Display | Integrate all display elements |
| 17E | F | Benchtop Simulation | System performance on bench |
| 18E | F | Functional | System performance installed |
| 19E | A | Timing | System response time |

Table 3. Web Interface Test Plan

| **#** | **L** | **Description** | **Tests function:** |
| --- | --- | --- | --- |
| 1W | U | Flask | Flask framework |
| 2W | U | SocketIO | SocketIO interactivity |
| 3W | U | Database | Save/Retrieve data |
| 4W | U | Network | Receive/Send UDP |
| 5W | I | Settings Page | Settings functions |
| 6W | I | Status Page | Status page |
| 7W | I | Network Commands | Send/Receive commands |
| 8W | I | Embedded | Embedded send/receive |
| 9W | F | Functional | System performance installed |

# Detail Design

## Traffic Simulators

Python scripts were written to simulate the traffic between the embedded system and the web interface. They simulated the messaging so that both subsystems could be built independently. The scripts enabled the unit testing of the network sending and receiving with only one subsystem available. This enabled both the web and the embedded system to be developed in decoupled timelines.

## Embedded System Software

The embedded system was divided into five periodic concurrent prioritized (P) tasks (3 is the highest) as shown in Table 4. The FreeRTOS uses priority based preemptive schedular. Scheduling frequency was selected based on the timing requirements identified earlier.

Table 4. Tasks, Priority, and Interval Time

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **Task** | **P** | **Hz** |
| 1 | TaskReadSensors | 3 | 100 |
| 2 | TaskUpdateDisplay | 1 | 2 |
| 3 | TaskPriorityMachines | 2 | 10 |
| 4 | TaskNetwork | 1 | 2 |
| 5 | TaskWatchdog | 1 | 0.67 |

When registered with the scheduler, a task control block and individual stack is allocated. The scheduler handles context switching and pulling tasks in and out of execution. The developer is responsible for handling access to shared resources using mutexes or queues. The GarageRTC employs four global mutexes for shared resources:

* *g\_sharedMemMutex* – protects shared memory and global variables
* *g\_serialMutex* – protects access to the serial port
* *g\_wdMutex* – protects access to the watch dog bowl

### Task Read Sensors

This task is responsible for fetching, converting values from the sensors and making the results available other tasks. The task runs every 10mS and has the highest priority in the system. It buffers data as it is being collected and then writes it back protected by the *g\_sharedMemMutex*. In general, this task implements the following functions:

* Fetch values from sensors
* Scale/Convert values
* Read/debounce switches
* Store values to memory
* Update shared variables

### Task Update Display

This task is responsible for updating the local display. The task runs every 500mS and has the lowest non-idle priority in the system. This task performs the following functions:

* Fetch values from memory
* Post readings or status to the display
* Calculates Door Position and System state for the web
* Update the displays including:
  + Temperature
  + CO Level
  + Connection Status
  + System state

### Task Priority State Machines

This task is responsible monitoring door position, obstacle detection, and starting or stopping movement. Light control and alaram state were also added into this task. The functions of each state machine are described in detail below. In general, this task performs the following functions:

* Maintain Door state
* Start/Stop door movement
* Monitor obstacle detection
* Operate the light state machine
* Operate the Alarm state machine

The light control state machine ensures proper latching the associated relay. The state machine takes button press state as an input. It includes dwell states where the user is holding down the button. Using the state machine documented in Figure 8 below, the button functions as a press-on and press-off latching output. The state machine prevents the relay from fluttering if the relay if the button is pressed and held for a length of time.




Figure 8. Light Control State Machine

The door control state machine operates the relay attached to the opener button. When the DOOR button is pressed on the GarageRTC or door web command, the state machine triggers the door switch for a period. Then it idles as the door moves. If the door strikes a limit switch or obstacle, another pulse is sent to the switch to stop the movement. If the user presses the stop button or a stop web command is sent, the machine moves to the stopping state. The state machine is shown in Figure 9.




Figure 9. Door Control State Machine

The alarm control state machine monitors the temperature and CO sensor against predetermined set points. When the limits are exceeded, the state machine sets the Alarm relay. If the user presses the Alarm button or Alarm web command is received, the alarm is silenced by opening the relay. The alarm state will persist until the value falls into the acceptable range with hysteresis. The state machine for the alarm control is shown in Figure 10.




Figure 10. Alarm Control State Machine

### Task Watchdog

The watchdog needs to monitor all tasks and ensure they are periodically operating. This is achieved by creating a bit-wise “Bowl” where each of tasks is required to set a flag at completion. An interrupt is registered on a timer set to 3 seconds. In the service routine of the ISR, a system reset is triggered. Periodically, the watchdog task will check the bowl. If all bits are set, then the watchdog resets the timer and empties the bowl. If the bowl is never completely full, such as when one tasks is starving or stuck, then watchdog never resets the timer, Figure 11. Eventually the timer exhausts and the system is reset, hopefully clearing the fault condition.




Figure 11. Watch Dog Operation

## Embedded System Hardware

The proof of concept hardware was built and assembled using off the shelf modular components, breadboard, and a backing board. The components were sourced and assembled using discrete wiring. The complete bill of materials is listed in Table 5. The following subsections describe the notable components including the microcontroller, CO Detector, and Display.

Table 5. Bill of Materials

|  |  |  |  |
| --- | --- | --- | --- |
| **REF** | **Part** | **PN** | **Qty** |
| U1 | ESP32\_NodeMCU | B07F877YZQ | 1 |
| U2 | 4x20 LCD Display | 030003LA | 1 |
| D1 | Laser Diode Assy | 1172 | 1 |
| D2 | Laser Detector | B01M8PFZRC | 1 |
| S1-S5 | Mom PCB Switch | B06XT3FLVM | 4 |
| S6-S8 | Limit Switch | V-153-1C25 | 2 |
| K1 | 4x Relay Assy | 4450182 | 1 |
| J1 | USB Cable | 7T9MV4 | 1 |
| CO | CO Detector | FTC010-MQ-7 | 1 |
| R1 | 10k Thermistor | MF52-103 | 1 |
| R2 | 10k ohm ±1% 1/4W | MFP-25BRD52-10K | 1 |
| - | Breadboard | B01EV6LJ7G | 1 |

### Microcontroller

The microcontroller selected is an Espressif ESP32 system-on-a-chip micro-controllers that utilizes the Tensilica Xtensa microprocessor. The specific development board selected is an NodeMCU-32S compatible which includes a USB to serial interface for re-programming and serial monitoring. The ESP32 is supported by the FreeRTOS project and a board support package is available for the Arduino IDE. The ESP32’s features include:

* Dual-core 32-bit processor
* Ultra-low power co-processor
* 25 GPIO, 6 Analog Input, and 2 Analog Output
* 3 UART, 3 I2C, and 2 SPI
* Cryptographic and security ASICS
* 4 MB of Flash, with 520 KB of SRAM
* Built in 802.11n Wi-Fi and Bluetooth LE
* Software, hardware, and timer interrupts




Figure 12. NodeMCU-32S Compatible ESP32 Module

### CO detector

For detection of Carbon Monoxide MQ-7 CO detector integrated onto a development module, Figure 13, that includes a comparator pre-amp. The module has an adjustable digital alarm output (not used) and a scaled analog output reporting parts per million of carbon monoxide.



Figure 13. MQ-7 Carbon Monoxide Detector

The challenge with the CO detector was calibration and susceptibility to temperature and moisture variation. The research team did not have a calibrated source for correcting the CO concentrations and the sensor was found to be sensitive to fluctuations in temperature and humidity. The sensor was ultimately rough calibrated by using ambient in-house CO readings as “LOW” and then “HIGH” on the tailpipe of a cold start automobile. The “WARN” threshold was set at approximately 20% of the observed full range and then adjusted to not trigger any warnings when operating in the home.

### Display

The display was initially selected to be a 0.91” 128x32 SPI OLED monochrome graphic display. There were several sources of drivers available for this type of display for the ESP toolchain. However, when the team attempted to integrate the drivers, they found that they were only partially functioning. After attempting to integrate the display, manually update drivers, and struggling through poor documentation, the team decided to return the high level design and select a different display.

Finally, a simpler to integrate 20 character by 4 line LCD display, Figure 14, was sourced and integrated. This display is a parallel matrix interfaced through a SPI to parallel PCF8574 remote 8-Bit I/O Expander for I2C Bus. Drivers already existed for this simple protocol and the display was quickly integrated. The display chemistry, however, has somewhat poor contrast and is slow to update.



Figure 14. 20x4 Character LCD SPI Display

### Obstacle Detection

For obstacle detection, the team considered interfacing with the breakbeam eyes supplied with conventional openers. Research revealed that these sensors typically emit an AC waveform that the opener looks at to ensure the sensor has not been bypassed. Ultimately, the teams selected a laser module and a laser detector diode pair as shown in Figure 15.






Figure 15. Laser Transmitter and Diode Detector

### Completed Proof of Concept GarageRTC Assembly

The fully integrated assembly was attached to a mount to provide rigidity and ease of portability. Mounting holes were added to allow the mechanism to be affixed to the wall temporarily for testing. The system used a standard 4 gang relay to provide mains switching and opener button control. Power was provided by means of a AC to USB adapter or from the laptop.



## Web Service

The web service was built constructed with three main pages:

* Menu page for navigating
* Status page for monitoring/commanding the system
* Settings page for configuring the system

The menu page, Figure 17, allows the user to navigate between the landing page (Home), Status, and Settings pages. It is accessed through the settings button in the upper right corner of the display.




Figure 16. Menu Page

For the Status page, the web service used python to capture and process JSON packages from the network interface. These were then stored to dictionaries within the Flask framework. JavaScript would then periodically read the data structure and update the user interface status page. An interval timer and button presses to the web user interface were processed by the JavaScript and fed to the Python data structure and signaled the Flask framework. When the event was processed, the python would create and send either a command or get status packet and write it to the network adapter to be sent to the embedded system. A data flow graph of the web server subsystem is shown in Figure 16 illustrating the process.




Figure 17. Data Flow Graph of the Web Server Subsystem

The interactive status page is shown in the figure below:




Figure 18. Status Page

The settings page, allows the user to configure the target GarageRTC IP address. The user can configure the IP and Port as well ad adjust the screen cycle time. This information is then written back to the database and used for sending/receiving to the target GarageRTC.




Figure 19. Settings Page

## Integration of Web and Embedded

Finally, the web and embedded sections were brought together for combined testing. The team encountered minor bumps in the integration as each team had made assumptions about how the other subsystem would operate. Some final integration modifications were made, and the web interface was used to exercise the embedded functions on the bench. The use of the interface defined early in the design phase and simulators developed to support testing had enabled quick and successful integration between the two subsystems.

## Unit Testing and Code Refinement

Testing consisted primarily of unit testing during development. Unit tests were used to proof out each component as it was incrementally added to the system. Eventually, as the system grew more complex and stable as features were added. Finally, the system could be tested as an assembly. Bench tests of the state machines and outputs were performed.

After the system was mostly integrated and functioning, a code baseline was established, and several rounds of performance tuning was performed. This consisted of moving variables out of the global space, reducing loop complexity, and minimizing memory usage. The remaining global variables were guarded by mutexes and local buffers established to ensure consistent operation. Several passes were made to remove dead code, simplify math, and reduce primitive data types, such as int to byte. Rather than dealing programmatically with strings, static char arrays were constructed to allow indexing into static arrays using integer enumerations. Debug statements and inaccessible code was removed.

# Testing

Functional testing consisted of walking through all the major functions on the device. First on the bench, then the unit was installed on a working garage door, Figure 20. Several minor software bugs were identified, and system timings were adjusted. A video of the major features of the GarageRTC was produced and uploaded to YouTube.




Figure 20. Functional Testing Installation

A model of the completed system with all submodules integrated into a single assembly was created, Figure 21. This model demonstrates that the packaging could be substantially reduced, and a neater, more professional packaging could be obtained.


**

Figure 21. Model of Integrated RTC Assembly

## Performance

Performance of the GarageRTC was measured in terms of utilization, memory usage, and measured response timing with respect to the original requirements.

### Utilization

Using an oscilloscope connected to the debug pins, the worst case timing of each task was captured. The frequency of scheduling was also captured. Using this information, the system utilization was computed to be approximately 8.4% utilized. This is considered extremely underutilized. However, the ESP32 may be overpowered for the scheduled tasks, the integrated WiFi is the big benefit.

Table 6. Utilization Calculation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Task** | **FMeas** | **ei** | **pi** | **ei/pi** |
| TaskReadSensors | 100 Hz | 29.5 uS | 0.01 | 0.00295 |
| TaskUpdateDisplay | 2 Hz | 39 mS | 0.5 | 0.078 |
| TaskPriorityMachines | 10 Hz | 1.41 uS | 0.1 | 1.41E-05 |
| TaskNetwork | 2 Hz | 2.015 mS | 0.5 | 0.00403 |
| TaskWatchdog | Varies | 1.05 uS | 0.67 | 1.58E-06 |
|  |  |  | **U =** | 0.084 |

For memory utilization, the current application uses approximately 720 kB bytes or 54% of program memory. Without Networking and UDP libraries, application consumed only approximately 15%. This means the network stack and UDP messaging consumes ~524 kB or almost 40% of program memory. Global variables use 38kB (11%) of dynamic memory leaving 290 kB for local variables which includes individual task stacks.

### Timing

For measuring system timing, the oscilloscope was attached to the input line from the switch and second channel attached to the output signal. The average of 10 presses was measured on the door button, stop button, light button, and obstacle sensor. The results were that switching occurred as quickly as 40 mS and never slower than 86.2 mS. The average response was around 58.6 mS. Worst case switching was still far better than the tightest requirement of 150 mS. The timing for LCD and network data was based on cycle time for the task using a debug pin toggling at the start and end of the task. The resulting timing against the requirements is shown below in Table 7.

Table 7. Timing Requirements and System Measurement

| **Parameter** | **Timing Requirement** | **Measurement** | **P/F** |
| --- | --- | --- | --- |
| Local Display | Every 500 mS or better | 500 mS | P |
| Obstacle Detection | Toggle opener within 150 mS from detection | < 86.2 mS | P |
| Limit Switch | Toggle opener within 150 mS from detection | < 86.2 mS | P |
| Door movement | Toggle opener within 300 mS from press | < 86.2 mS | P |
| Light | Latch light within 300 mS from press | < 86.2 mS | P |
| Idle Post to Server | Post to the server every 5000 mS | 500 mS | P |
| Event push to server | Post to the server within 500 mS from event. | <= 500 mS | P |
| Check Server | Check remote messages every 1000 mS | 500 mS | P |

# Accomplishments and Limitations

## Objectives Met

After reviewing the requirements as defined in the original project proposal, all objectives that were established at the outset of this project were met. Table 8 contains the completed requirements matrix.

Table 8. GarageRTC Requirement Compliance

|  |  |  |
| --- | --- | --- |
| **Requirement** | **Description** | **Met?** |
| ECE554-REQ-001 | Manual Interface Switches | Yes |
| ECE554-REQ-002 | Local Display | Yes |
| ECE554-REQ-003 | Light Control | Yes |
| ECE554-REQ-004 | Sensing Requirements | Yes |
| ECE554-REQ-005 | IoT Connectivity | Yes |
| ECE554-REQ-006 | Web Service | Yes |
| ECE554-REQ-007 | Timing Requirements | Yes |

## Limitations

The system does have a couple minor limitations. The first is that the alarm push notifications to the server were combined into the same task as the regular network update task. This means that the best possible response time will be governed by the update time of TaskNetwork. Further, there is stacked delay between the reception of the UDP packet and publishing to the page. This seems to work well in practice, but for more responsive alerts more tuning should be put into an asynchronous push from the embedded system and fine tuning the cycle time of the web server.

Secondly, the carbon monoxide detector was not able to accurately be calibrated. The sensitivity to moisture and temperature means that the calculation for the CO is a function of temperature and humidity. While temperature is available, humidity was not. Temperature measurement was accomplished by use of a glass bead thermistor and the regulated 3.3VDC rail. Good for gross measurement of temperature but if incorporated into the CO calculation, could make the CO output unreliable. The gross calibration of the CO sensor seems to be mostly sufficient, but occasionally will trigger CO false positives when the garage temperature drops below 50 F.

## Lessons Learned

## Possible Improvements

The project made several design decisions in the interest of simpler development. To ease network integration, the system employs UDP and no encryption. These are considered experimentation only type configurations and would need to be resolved in a more production ready version of the product. The system also interfaces to the garage door lift motor through the operator button, this too could be improved. Finally, the system depends on the obstacle sensor being well aligned and can easily be spoofed by jumpering the signal wires. This section discusses potential improvements to solve these issues intended in a future revision of the GarageRTC project.

UDP simplifies the design by reducing the network configuration within the web app and embedded unit, but routing traffic to any area larger than the immediate subnet is impractical. The excessive packets will hinder network congestion and are not easily forwarded to another network if the server was not on the same subnet. To solve this, the system should be moved over to TCP based networking between the server and GarageRTC. This would also more easily enable security features such as TLS.

The lack of encryption is certainly simplified design by not having to create, manage keys, and develop paring processes for the server and embedded unit. Obviously in this day an age, any IoT device is under heavy scrutiny from security researchers. With the current design, anyone on the network could easily replay a packet and get the garage door to move. The solution would involve adding application layer encryption between the embedded and server. For further protections, TLS could also be added by embedding certificates that are mutually authenticated.

Another limitation is that the GarageRTC interacts with the garage door lift motor through the opener button interface. Each garage door operates a little differently, such as longer button pulses or automatic reversing after a down trigger. This makes the interaction between the GarageRTC and the opener not ideal. A potential solution would be to incorporate a direct dive reversable H-Bridge controller into the project. That would give the controller better control over the door. The downside is there are significant safety impacts that need to be considered when taking over control of the door lift mechanism.

Lastly, the laser transmitter and receiver used by the project could be improved by replacing it with a pair of conventional garage break beam eyes. These devices typically use a proprietary protocol but do incorporate anti-spoof circuitry, so the door controller can tell if they have been intentionally jumpered. They also are more tolerant of misalignment. Replacing the laser with libraries to interface with different conventional eyes would reduce system cost, improve safety, reliability, and performance.

Add section about moving the web server inside the ESP itself, Integrating with Alexa, android app, logins….

Further testing?

# Comparison of Commercial Offerings

Several commercial IoT garage devices are available to consumers. These devices are typically developed by major opener manufacturers and marketed as an upgrade to the existing opener electronics. This section provides a short review of several of these offerings and their compatible hardware. Surprisingly, none of these technologies offered native integration with digital assistants such as Amazon Alexa. We provide a comparison between the GarageRTC features and the commercial offerings and discuss the benefits and drawbacks of these paired solutions.

This section provides a short review of several of these offerings and their compatible hardware. Surprisingly, none of these technologies offered native integration with digital assistants such as Amazon Alexa. We provide a features comparison between the GarageRTC and commercial offerings reviewing the benefits and drawbacks of these paired solutions.

## Commercial IoT Garage Interfaces

The market was surveyed for commercial IoT garage interfaces that offer similar capabilities as to what was implemented for the GarageRTC project. The two most prominent opener companies, Chamberlain and Genie, offered hardware designed to interface with their respective openers. There was also a couple of notable general-purpose add-on modules designed to interface with a variety of openers. There were several minor part number differences, but the technologies surveyed were grouped as follows:

* Chamberlain MYQ-G0301
* Aladdin Connect
* Garage Door Buddy
* GoControl GD00z-4

## Comparison with GarageRTC Features

Next the team created collected documentation publicly available from the device’s respective marking pages. From this the research team composed a matrix considering connectivity, digital assistant integration, sensing and control, local interface, and openness of design. The compiled data is summarized in Table 6 below. References to the respective manufacturer’s site is included in the appendix of this document.

Table 9. Comparison of Commercial Devices

| **Feature** | MYQ-G301 | Aladdin Connect | Door Buddy | GoControl | GarageRTC |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Connectivity** |  |  |  |  |  |  |
| WiFi | ✔ | ✔ | ✔ |  | ✔ |  |
| Bluetooth |  |  |  |  | *1* |  |
| ZWave |  |  |  | ✔ |  |  |
| **Digital Assistant** |  |  |  |  |  |  |
| Alexa |  |  |  |  | *2* |  |
| Google |  |  |  |  | *3* |  |
| Siri |  |  |  |  | *3* |  |
| **Sense/Control** |  |  |  |  |  |  |
| Aux Control | *4* |  |  |  | ✔ |  |
| Amb. Temp |  |  |  |  | ✔ |  |
| Amb. CO |  |  |  |  | ✔ |  |
| Door Position | ✔ | ✔ | ✔ | ✔ | ✔ |  |
| **Local Control** |  |  |  |  |  |  |
| LCD Display |  |  |  |  | ✔ |  |
| Door | ✔ | ✔ | ✔ | ✔ | ✔ |  |
| Aux/Light |  |  |  |  | ✔ |  |
| **Open Source** |  |  |  |  |  |  |
| Web App |  |  |  |  | ✔ |  |
| FOSS |  |  |  |  | ✔ |  |
| Published API |  |  |  |  | ✔ |  |
| HW Schematic |  |  |  |  | ✔ |  |
| Universal |  |  | ✔ | ✔ | ✔ |  |
| **Reference** | [9] | [10] | [11] | [12] |  |  |
| 1. ESP32 contains the hardware but reference design does not implement.  2. Libraries exist that could integrate this capability. [13]  3. Can be integrated through webhook/REST API calls. [14]  4. Requires purchase of additional hardware. | | | | | | | |

## How GarageRTC differs from current solutions

The GarageRTC is comparable to commercial offerings in all categories and is stand-out in design openness. The open source nature of the GarageRTC makes it considerably more adaptable and extensible than the consumer offerings.

It is important to note that security was omitted from the table. The team found that, while the manufacturers advertised various “security assurances” they did not publish details on how these were achieved. The GarageRTC does not currently employ any sort of link encryption and depends completely on the security of the wireless access point. The team expected the security category to be the location where the commercial offerings would outshine the project. However, since the details of their security mechanisms could not be determined, it is difficult to say if the commercial systems are offering much more than security through obscurity. The research work done by J. Margulies, C. Goudie and R. Weidner, indicate verifying levels of security effectiveness. [15] [16] For these reasons, the security offerings cannot be effectively compared without a more thorough evaluation. A proposal for security on the GarageRTC project can be found in section VII.D of this paper.

The commercial offerings did have the advantage in that they tended to offer applications with credentials. All solutions surveyed offered Android and IOS native apps for their remote interface. Frequently, these applications are merely application wrapping around a web interface. This simplifies development and can help with security if the site is properly protected. The location of the IoT service could not be conclusively determined from the documentation surveyed, but it is reasonable to assume that it is most likely a closed source cloud hosted service. If the support for the cloud service is suspended, then these devices would likely fail to function. Since the GarageRTC hosts a generic web page, it’s reasonable to say that the GarageRTC offers equivalent performance.

## Benefits and drawbacks of the integrated solution

The primary benefit of the commercially available devices is they have corporate backed development support. This translates to more refined software and user-friendly interfaces as they have superior developer resources as compared to the GarageRTC research team. They have the capacity to fully implement and test their solutions and maintain professional assistance hotlines. Further, mass production of their assemblies’ results in greater availability and prices typically ranging from $50 to $100. However, if the popularity of GarageRTC caught on, the resulting user community could quickly make up this gap. Further development could produce layouts to meet off the shelf housings or 3D printed enclosures.

The major drawbacks of the commercial units are their closed source nature. Vulnerabilities have been identified in the garage door solutions and countless other issues may exist. [15] These units have not undergone any sort of security community analysis and publish very little documentation on security controls available. The GarageRTC, however, doesn’t currently employ any security as it was not the focus of this effort, could easily have any flavor of security controls the developer prefers. Since the source is open, the security community could then review the implementation, identify potential flaws and make recommendations for remediation.

The closed source communication protocols also mean that the lifetime of these products is directly tied to the supplier’s willingness to continue support. If the companies go out of business or cease support in favor of a newer generation part, customers will be out of luck. The GarageRTC project offers the ability for anyone to stand up or share their own web application servers and therefore can indefinitely support hardware built to meet the GarageRTC protocols.

# Conclusions and Closing Remarks

The GarageRTC met most of the performance and design requirements as identified in the concept and requirements phase. The system was more than capable of proving responsive interactivity with a residential garage door system.

The high-level design outlined an organized approach to system development during the integration phase. The test plan outlined and iterative updates to the user’s manual kept development on track and features aligned with the original intent. The ESP based hardware and Arduino IDE performed will when coupled with the FreeRTOS OS for the embedded system. Flask, JavaScript, and socketio simplified development of the web interface and packet engine interface to the embedded system.

Detailed design produced detailed state machines prior to implementation and helped align runtime tasks with desired functional behavior. The OLED display was identified early to not meet desired performance and the 20x4 character LCD was substituted with minimal re-work. The network simulators developed allowed the development timelines of the embedded system and the web to be decoupled. Integration of the web and embedded portion was eased by use of the simulators and early established network commands interface.

Unit testing proofed out component functionality independently allowing the research team to revalidate hardware periodically. This also ensured that both team members were aligned when implementing the hardware. Extensive bench testing ensured that only minor issued were encountered when installing the completed system in the intended environment.

The system was functionally benchmarked against other commercial offerings. The flexibility of the GarageRTC platform enables it to outperform its commercial counterparts. Although the GarageRTC did not implement security within its design, the other systems did not offer details on their security.

This paper set out to reviews the features, design, and implementation of a reference architecture built on an ESP32 microcontroller and FreeRTOS software. The materials created during this effort have been posted publicly and freely available. The researchers believe this proof of concept firmly demonstrates that open source IoT products are viable and can offer similar performance to a commercial product but without the burden of developing and maintaining dedicated closed source cloud services.

# References

|  |  |
| --- | --- |
| [1] | A. Zeichick, "Throwing our IoT investment in the trash thanks to NetGear," *Network World,* 11 July 2016. |
| [2] | J. Perlow, "When your IoT goes dark: Why every device must be open source and multicloud," *ZDNet,* 12 March 2019. |
| [3] | S. Levin, "Squeezed out: widely mocked startup Juicero is shutting down," *The Guardian,* 1 September 2017. |
| [4] | R. Suehle, "Q. What is the secret of Red Hat's Success?," *Technology Innovation Management Review,* January 2012. |
| [5] | R. Barry, "Mastering the FreeRTOS Real Time Kernal," Real Time Engineers Ltd, 2016. |
| [6] | H. Gochkov and I. Grokhtkov , "Arduino core for ESP32 WiFi chip," 20 January 2019. [Online]. Available: https://github.com/espressif/arduino-esp32. [Accessed 20 March 2019]. |
| [7] | A. Ronacher, "Flask a microframework for Python," The Pallet Project, 20 April 2019. [Online]. Available: https://www.palletsprojects.com/p/flask/. |
| [8] | G. Rauch, "Socket.IO," Automattic, 20 April 2019. [Online]. Available: https://socket.io/. |
| [9] | Chamberlain, "MYQ Smart Garage Hub," Chamberlain, 2019. [Online]. Available: https://www.chamberlain.com/myq-smart-garage-hub/p/MYQ-G0301-D. [Accessed 13 April 2019]. |
| [10] | Genie, "Aladdin Connect," Genie, 2019. [Online]. Available: https://www.geniecompany.com/aladdinconnect/default.aspx. [Accessed 13 April 2019]. |
| [11] | GarageDoorBuddy, "GarageDoorBuddy - Remotely Control your garage doors from Anywhere," Garage Door Buddy, 2019. [Online]. Available: http://garagedoorbuddy.com/. [Accessed 13 April 2019]. |
| [12] | GoCOntrol, "GD00Z-4: Z-Wave Garage Door Opener Remote Controller Accessory," GoControl, 2019. [Online]. Available: http://www.gocontrol.com/detail.php?productId=4. [Accessed 13 April 2019]. |
| [13] | X. Pérez, "FauxmoESP - Amazon Alexa support for ESP8266 and ESP32 devices," 2019. |
| [14] | X. Pérez, "Using Google Assistant to control your ESP8266 devices," Tinkerman, 2019. [Online]. Available: https://tinkerman.cat/using-google-assistant-control-your-esp8266-devices/. [Accessed 13 April 2019]. |
| [15] | J. Margulies, "Garage Door Openers: An Internet of Things Case Study," *IEEE Security & Privacy,* 2015. |
| [16] | C. Goudie and R. Weidner, "Home hackers: Digital invaders a threat to your house," *ABC 7 News, Chicago IL,* 12 February 2015. |
| [17] | J. P. Pawar, S. Amirthaganesh, S. ArunKumar and K. B. Satiesh, "Real Time Energy Measurement using Smart Meter," in *Online International Conference on Green Engineering and Technologies (IC-GET)*, Online, 2016. |